|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| S.N. | DESCRIPTION OF ITEMS WITH SPECIFICATIONS | UNITS & QUANTITY | RATE  PER SQ.FT | AMOUNT |
| 1 | **BRICK WALL**  **25 CMX 12 CM X 8 CM FLY-ASH BRICKS (1:6) SUPER- STRUCTURE**  PROVIDING FLY ASH BRICK MASONRY WORK IN SUPER- STRUCTURE USING ( **25 CMX 12 CM X 8 CM SIZE) HAVING CRUSING STRENGTH NOT LESS THAN 75KG/SQ CM IN CEMENT MORTAR (1:6) USE WITH ALL NECESSARY PROJECTIONS, SPLAYS CUTTING, CIRCULAR MOULDING, CORBELLING ETC AS PER DRAWINGS, INCLUDING COST, COVEYANCE, ALL TAXES, ROYALITIES, LOADING AND UNLOADING OF ALL MATERIALS, INCLUDING COST OF ALL LABOUR, SCAFFOLDING, WATERING AND CURING, SUNDRIES, TOOLS &PLANTS ETC.COMPLETE AS PER THE DIRECTIONOF THE UNDERSIGNED.** |  |  |  |
| 2 | **CEMENT PLASTERING ( 16 MM THICK PLASTER )**  PROVIDING 16 MM (5/8 INCHES) THICK CEMENT PLASTER (1:6) IN ALL FLOORS AND WALLS FINISHED SMOOTH TO INSIDE AND OUTSIDE ROUGH SURFACE AFTER RACKING OUT THE JOINTS INCLUDING **COST, COVEYANCE, ALL TAXES, ROYALITIES, LOADING AND UNLOADING OF ALL MATERIALS, INCLUDING COST OF ALL LABOUR, SCAFFOLDING, WATERING AND CURING, SUNDRIES, TOOLS &PLANTS ETC.COMPLETE AS PER THE DIRECTIONOF THE UNDERSIGNED.** |  |  |  |
| 3 | **RCC(REINFORCED CEMENT CONCRETE) M20** WITH CENTERING AND SHUTTERING  REPAIRS TO RCC MEMBERS SUCH AS COLUMNS, BEAMS, SLABS, ETC. INCLUSIVE OF MAKING OF DAMAGED AREAS, CHIPPING OFF LOOSE AND DISINTEGRATED CONCRETE, PREPARING EXPOSED CONCRETE AS SPECIFIED, CLEANING THE REINFORCEMENT WITH WIRE BRUSH, CHIPPING HAMMER AND PROTECTIVE COATING OF KP-100 ON CONCRETE NEAR THE EXPOSED STEEL,ANTICORROSIVE COATING OF IPNET RB ON OLD AS WELL AS NEW STEEL, BOND COAT OF EL MONOBOND ON CONCRETE INTERFACE, RESTORING ALL BROKEN CONCRETE BY POLYMER MODIFIED CONCRETE IN (MIX 1:3) (1 PARTS OF CEMENT :3 PARTS OF GODHRA SAND) WITH 5 KG OF MONOBOND (OF SIKA OR APPROVED BRAND) PER BAG OF CEMENT, OF ANY THICKNESS AND CURING ETC. COMPLETE ALL AS SPECIFIED AND/OR AS DIRECTED BY THE CONSULTANT, BUT EXCLUDING NEW REINFORCEMENT AS NECESSARY, DOWELS/SHEAR PINS, PLASTER FINISH AND GROUTING CONCRETE MATRIX WHICH ARE PAID SEPARATELY. |  |  |  |
| 4 | **WATER PROOFING (GRADING)**  PROVIDING AND LAYING INTEGRAL CEMENT BASED WATER PROFFING TREATMENT INCLUDING PREPARATION OF SURFACE AS REQUIRED FOR TREATMENT OF ROOFS, BALCONIES, TERRACES ETC, CONSISTING OF FOLLOWING OPERATIONS. A) SUPPLYING AND APPLYING TWO COATS OF ACRYLIC POLYMER BRUSH BOND (TWO PARTS SYSTEM) OVER THE PREPARED SURFACE. THE ITEM IS CONSISTS OF A POWDER COMPONENT AND PREMEASURED LIQUID COMPONENT. WHICH SHALL BE MIXED AS PER MANUFACTURE’S INSTRUCTION AND SHALL BE APPLIED.  B) TREATED SURFACE OF BRUSH BOND SHOULD BE COVERED BY CEMENT MORTAR AVERAGE THICKNESS OF 25MM BY GIVING A PROPER SLOPE BY USING CONPLAST X421IC (INTEGRAL WATERPROFFING COMPOUND ) AT A DOSAGE OF 125ML PER BAG OF CEMENT AS PER IS:2645 ADJOINING WALLS UP TO 150 ML HEIGHT INCLUDING ROUNDING OF JUNCTIONS OF WALLS AND SLABS. |  |  |  |
| 5 | **FLOOR TILES**  SUPPLYING AND FIXING PREMIUM QUALITY CERAMIC FLOOR AND WALL TILES OF APPROVED COLOUR AND SHADE, MAKE AS KAJARIA, JOHNSON, SOMANY SIZE OF 300MM X300MM IN ALL COMPLETE. |  |  |  |
| 6 | **WALL TILES**  SUPPLYING AND FIXING PREMIUM QUALITY CERAMIC FLOOR AND WALL TILES OF APPROVED COLOUR AND SHADE, MAKE AS KAJARIA, JOHNSON, SOMANY SIZE OF 300MM X450MM IN ALL COMPLETE. |  |  |  |
| 7 | **PAVER BLOCKS**  SUPPLYING AND LAYING M 60 PAVER BLOCK WITH 2.5’’ SAND FILLING LABELLING, WATERING AND CONCRETING IN ALL COMPLETE. |  |  |  |
| 8 | **WEATHER PAINTS (WITH MATERIAL)**  PROVIDING & PAINTING TWO COATS WITH WATER SOLUBLE WEATHER COAT PAINT AND PUTTY REPAIRING OF APPROVED SHED (ASIAN AND BURGER ) TO OUTSIDE BRICK WALL OVER A COAT OF CEMENT WASH AND PRIMING BY MEANS OF BRUSH TO OUT SIDE SURFACE OF A NEW WALL AFTER SCRAPPING CLEANING THE SURFACE INCLUDING COST OF MATERIALS, SCAFFLODING , LABOUR, WATERING, CURING TOOLS & PLANTS ETC. COMPLETE THE DIRECTIONS OF UNDERSIGNED. |  |  |  |
| 9 | **WEATHER PAINTS(WITHOUT MATERIAL)**  PROVIDING & PAINTING TWO COATS WITH WATER SOLUBLE WEATHER COAT PAINT AND PUTTY REPAIRING OF APPROVED SHED (ASIAN AND BURGER ) TO OUTSIDE BRICK WALL OVER A COAT OF CEMENT WASH AND PRIMING BY MEANS OF BRUSH TO OUT SIDE SURFACE OF A NEW WALL AFTER SCRAPPING CLEANING THE SURFACE INCLUDING COST OF MATERIALS, SCAFFLODING , LABOUR, WATERING, CURING TOOLS & PLANTS ETC. COMPLETE THE DIRECTIONS OF UNDERSIGNED |  |  |  |
| 10 | **DISTEMPER PAINTS (WITH MATERIAL)**  PROVIDING & PAINTING TWO COATS WITH WATER SOLUBLE DISTEMPER PAINT AND PUTTY REPAIRINGOF APPROVED SHED (ASIAN AND BURGER) TO INSIDE BRICK WALL OVER A COAT OF CEMENT WASH AND PRIMING BY MEANS OF BRUSH TO OUT SIDE SURFACE OF A NEW WALL AFTER SCRAPPING CLEANING THE SURFACE INCLUDING SCAFFLODING, LABOUR, WATERING, CURING TOOLS & PLANTS ETC. COMPLETE THE DIRECTIONS OF UNDERSIGNED. |  |  |  |
| 11 | **DISTEMPER PAINTS(WITHOUT MATERIAL)**  PAINTING TWO COATS WITH WATER SOLUBLE DISTEMPER PAINT AND PUTTY REPAIRINGOF APPROVED SHED (ASIAN AND BURGER) TO INSIDE BRICK WALL OVER A COAT OF CEMENT WASH AND PRIMING BY MEANS OF BRUSH TO OUT SIDE SURFACE OF A NEW WALL AFTER SCRAPPING CLEANING THE SURFACE INCLUDING COST OF MATERIALS, SCAFFLODING, LABOUR, WATERING, CURING TOOLS & PLANTS ETC. COMPLETE THE DIRECTIONS OF UNDERSIGNED. |  |  |  |
| 12 | **ENAMEL PAINTS (WITH MATERIAL)**  PROVIDING & PAINTING TWO COATS WITH SYNTHETIC ENAMEL PAINT AND PUTTY REPAIRING OF APPROVED SHED (ASIAN AND BURGER ) TO INSIDE BRICK WALL OVER A COAT OF CEMENT WASH AND PRIMING BY MEANS OF BRUSH TO OUT SIDE SURFACE OF A NEW WALL AFTER SCRAPPING CLEANING THE SURFACE INCLUDING COST OF MATERIALS, SCAFFLODING , LABOUR, WATERING, CURING TOOLS & PLANTS ETC. COMPLETE THE DIRECTIONS OF UNDERSIGNED. |  |  |  |
| 13 | **ENAMEL PAINTS(WITHOUT MATERIAL)**  PAINTING TWO COATS WITH SYNTHETIC ENAMEL PAINT AND PUTTY REPAIRING OF APPROVED SHED TO INSIDE BRICK WALL OVER A COAT OF CEMENT WASH AND PRIMING BY MEANS OF BRUSH TO OUT SIDE SURFACE OF A NEW WALL AFTER SCRAPPING CLEANING THE SURFACE INCLUDING SCAFFLODING, LABOUR, WATERING, CURING TOOLS & PLANTS ETC. COMPLETE THE DIRECTIONS OF UNDERSIGNED. |  |  |  |
| 14 | **SYNTHETIC PLASTIC PAINTS (WITH MATERIAL)**  PROVIDING & PAINTING TWO COATS WITH SYNTHETIC PLASTIC PAINT AND PUTTY REPAIRING OF APPROVED SHED (ASIAN AND BURGER) TO INSIDE BRICK WALL OVER A COAT OF CEMENT WASH AND PRIMING BY MEANS OF BRUSH TO OUT SIDE SURFACE OF A NEW WALL AFTER SCRAPPING CLEANING THE SURFACE INCLUDING COST OF MATERIALS, SCAFFLODING, LABOUR, WATERING, CURING TOOLS & PLANTS ETC. COMPLETE THE DIRECTIONS OF UNDERSIGNED. |  |  |  |
| 15 | **SYNTHETIC PLASTIC PAINTS (WITHOUT MATERIAL)**  PAINTING TWO COATS WITH SYNTHETIC PLASTIC PAINT AND PUTTY REPAIRING OF APPROVED SHED TO INSIDE BRICK WALL OVER A COAT OF CEMENT WASH AND PRIMING BY MEANS OF BRUSH TO OUT SIDE SURFACE OF A NEW WALL AFTER SCRAPPING CLEANING THE SURFACE INCLUDING SCAFFLODING, LABOUR, WATERING, CURING TOOLS & PLANTS ETC. COMPLETE THE DIRECTIONS OF UNDERSIGNED. |  |  |  |
| 16 | **CHECKUP TILES**  SUPPLYING AND FIXING PREMIUM QUALITY CHECKUP FLOOR TILES OF APPROVED COLOUR AND SHADE, MAKE AS SIZE OF 300MM X300MM IN ALL COMPLETE. |  |  |  |
| 17 | **PCC(PLAIN CEMENT CONCRETE)**  1:3:6 USING 4MM SIZE BHCB GRANITE STONES MENTALS INCLUDING WATERING CURING ETC IN ALL COMPLETE. |  |  |  |
| 18 | **SLIDING WINDOW ALUMINIUM**   |  |  | | --- | --- | | SUPPLYING AND FIXING TWO TRACK POWDER COATED GLAZE ALUMINIUM SLIDING WINDOW MADE WITH FRAME OF 40MM X 20MM FOR EACH LEAF AND FIXED FRAME OF 60MM X 30MM FIXED TO THE WALL WITH ALL FIXED ACCESSORIES LIKE **5MM THICK GLASS**, EDPM GASKET, HANDLES ETC.REQUIRED TO COMPLETE THE WORK. REPLACEMNT OF EXISTING GLASS WINDOWS. | **Rate**  **JINDAL** | | **ALAM** | | SUPPLYING AND FIXING TWO TRACK POWDER COATED GLAZE ALUMINIUM SLIDING WINDOW MADE WITH FRAME OF 40MM X 20MM FOR EACH LEAF AND FIXED FRAME OF 60MM X 30MM FIXED TO THE WALL WITH ALL FIXED ACCESSORIES LIKE **6MM FIBER**, EDPM GASKET, HANDLES ETC.REQUIRED TO COMPLETE THE WORK. REPLACEMNT OF EXISTING GLASS WINDOWS. | **JINDAL** | | **ALAM** | |  |  |  |
| 19 | **FLUSH DOOR 30MM**  SUPPLYING AND FIXING 30 MM THICKNESS FLUSH DOOR FINISHED WITH 6MM THICK TEAKWOOD LIPPING ON ALL EDGE, DULY POLISHED, 3 SS HINGES, 1 DOOR STOPPER, 2 HANDLES AND 1 MM LAMINATED BOTH SIDES IN ALL COMPLETE. |  |  |  |
| 20 | **PVC DOOR 28MM**  SUPPLYING AND FIXING 20MM THICK PVC DOOR INCLUDING HINGES, 2 HANDLES IN ALL COMPLETE. |  |  |  |
| 21 | **WELDING**  LABOUR FOR FITTING AND FIXING OF FABRICATION CHARGE, WELDING CHARGE ON LABOUR TOOLS AND PLANTS ETC. |  |  |  |
| 22 | FIXING OF 5MM CLEAR GLASS SAINT-GLOBIN FIXING WITH PUTTY WITH MATERIALS, TRANSPORTATION, LABOUR AND GST IN ALL COMPLETE. |  |  |  |
| 23 | FIXING OF 5MM CLEAR GLASS SAINT -GLOBIN FIXING WITH SILICON WITH MATERIALS, TRANSPORTATION, LABOUR AND GST IN ALL COMPLETE. |  |  |  |
| 24 | FIXING OF 5MM FIBRE SHEET AKMY WITH PUTTY WITH MATERIALS, TRANSPORTATION, LABOUR AND GST IN ALL COMPLETE |  |  |  |
| 25 | FIXING OF 5MM FIBRE AKMY FIXING WITH SILICON WITH MATERIALS, TRANSPORTATION, LABOUR AND GST IN ALL COMPLETE |  |  |  |